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Model Description for Piezo switch
For  example:NK16A-PNOF-EB12V/As
	*	■	□	...	6	♦	◊

	ff
plezo switch
code
	JLR-t
Mounting hole size
	
Type
	fl *llx
Head shape
	H;t:ffi: Switch combination
	t,\H'l=: rn Operation types
	*!l:T Lamp types
	!1:TTSl<Wi !Mi'M
LED color
/Button color
	!l:TT* ff
LED voltage
	91'
Housing

	
	12 <t:>12mm
	A
	p
	NO
	F:Momentan
	Blank
	Blanlc Non-ibum. B: Blue
G: Green Y: Yellow R:Red W:white
RG: Red/Green RY: Red/Yellow RB: Red/Blue RW: Red/White GB: Green/Blue GY: Green/Yellow GW: Green/White BY: Blue/Yellow YW: Yellow/White RGB: R/G/B RGY: R/G/Y RGW:R/G/W RBY: R/B/Y RBW:R/B/W RYW: R/Y/W GBY: G/B/Y GBW:G/B/W GYW:G/Y/W
BYW: B/Y/W
	SV(DC)
	As

	
	16 <!J16mm
	B
	P1
	NC
	(2 wire leads
	E
	
	12V(DC)
	Ab

	
	19 <!J19mm
	C
	P2
	K (proto-
	
	EO
	
	24V(DC)
	Aa

	
	22 <t:>22mm
25 <!J25mm
28 <!J28mm
30 <!J30mm
	D E
......
	
	
	
	
	
	
	

	
	
	
	PY
	
	
	
	
	
	s

	
	
	
	PZ
	
	
	
	
	
	


i1: iwfHIHmlw:.1" .F wi1H1*, -. :flUJ.s liil.F ttJ x tE**q:iii£ijW:Im1-\::-&o
Note: Please read carefully product detailed information,according to different product structure state in the table select the corresponding code.
* Head Shape:
P	=Flat, operator heighe 12mm=1.5, 16/19/22/25/30mm=1.30(non-illum)
P1	=Flat, operator height 4.50(16mm only)
P2	=Flat, operator height 3.00(not available with ring illum.)
PS	=Operator with finger location, height 12mm=1.5, 16mm=4.50(non-illum.) P6	=Finger location, operator height 3.00(not available with ring ilium.)
PA	=Chamfer, operator height 3.00(19mm only)
PY	=Chamfer, operator height 4.S0(available with thin or large ring ilium only) PZ	=Flat, operator height 4.S0(available with thin or large ring illum only)
The operator can be customized

.A. Operation types: Blank =Non-ilium
E	=Ring for operater 13.5 EO  =Ring for operater 16.5 D	=Dot


l*w 1:mooSurface Effect \ 










Notice:
· 
Housing:
As	=Natural anodized Ab =Blue anodized Aa =Black anodized Ag =Green anodized Ay	=Gold anodized Ar	=Red anodized
S	=Stainless steel 316L

1. The latching functions is with 3 or 4 wire leads
2. 12mm switch is with NO only,NOT for 3 wire leads
3. Standard Accessories supplied: 1 hex and 1 O-ring
4. Custom marking available
5. Ratings: 200mA 24VAC/DC
(1A 24VAC/DC is available) For options not listed,please contact us.
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Bushing/operator All models with <D 12 bushing
 (
Cw
®
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Flat

Finger location

P5	Operator with finger location. Blank		Flat operator, height 1,20(.047)
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Bushing/operator All models with <D 16 bushing







16A-P1NOF


<I> 18.00	o



Flat

Finger location

P1	 Flat operator, height 4,50(.177) p5	Operator with finger location.
height 4,50(.177)(non-illuminated)

Blank	Flat operator, height 1,30(.051)
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<I> 16.00 x 1.00 SI
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Bushing/operator

All models with <D 16 bushing

Flat operator, height 1,30(.051)

Flat




16A-PNOF-D
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t <D 16.00 x 1.00 SI (.630DIA x 1.00 IS)

IED
<D3.00 (.11SDIA)


3.70
(.146)







Bushing/operator

All models with <D 16 bushing

Flat operator, height 4,50(.177)
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<ll 16.00 x 1.00 SI (.630DIA x 1.00 IS)
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Bushing/operator




Flat

All models with CD 19 bushing
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Chamfer


P2 PA

Blank

Flat operator, height 3,00(.118)

Operator with chamfer, height 3,00(.118)
Flat operator, height 1,30(.051)
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Bushing/operator




Flat


All models with CD 19 bushing

Flat operator, height 1,30(.051)
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Bushing/operator

All models with CD 19 bushing


Flat	P2
PA
Chamfer

Flat operator, height 3,00(.118) Operator with chamfer,
height 3,00(.118)
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Bushing/operator All models with CD22 bushing




Flat

P2	Flat operator, height 3,00(.118)(non-illum.)
P6	Finger location,operator height 3,00(.118)(non-illum.) Blank		Flat actuator, height 1,30(.051)


Finger location

22A-P2NOF



(1)25.00
	(.984DIA)	











(!)20.50
(.807DIA)

(!)28.00 (1.102DIA)
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)<D 22.00 x 1.00 SI		 (.866DIA x 1.00 IS)
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Bushing/operator







Flat

All models with <D22 bushing
P2	Flat operator, height 3,00(.118)(non-illum.)
P6	Finger location,operator height 3,00(.118)(non-illum.) Blank	Flat operator, height 1,30(.051)

Finger location
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Flat Chamfer

P2	P6

Bushing/operator All models with <D22 bushing
PY	With chamfer, operator height 4,5mm (.177).
or large illuminated ring only
PZ	Flat operator, height 4,5mm (.177). or large illuminated ring only
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Bushing/operator

All models with <D25 bushing

P2	Flat operator, height 3,00(.118)(non-illum.)
P6	Finger location.operator height 3,00(.118)(non-illum.) Flat	Blank	Flat operator, height 1,30(.051)
Finger location

25A-P2NOF
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P6


Bushing/operator

All models with <D25 bushing

P2	Flat operator, height 3,00(.118)(non-illum.)
P6	Finger location,operator height 3,00(.118)(non-illum.) Flat	Blank	Flat operator, height 1,30(.051)
Finger location
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Bushing/operator





Flat Chamfer

All models with <D25 bushing
py	With chamfer.operator height4,5mm(.177) or large illuminated ring only
pz Flat operator, height 4,5mm(.177) or large illuminated ring only
Blank	Flat actuator.height 1,30(.051)
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Bushing/operator All models with <D30 bushing
P2	Flat operator, height 3,00mm(.118)(non-illum.)
P6	Flat location,operator, height 3,00mm(.118)(non-illum.) Flat	Blank	Flat actuator.height 1,30(.051)
Chamfer
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Bushing/operator All models with <l>30 bushing



Flat
Finger location
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P2	Flat operator, height 3,00(.11S)(non-illum.)
P6	Finger location.operator height 3,00(.11S)(non-illum.) Blank	Flat operator, height 1,30(.051)
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Bushing/operator All models with <l>30 bushing




Flat Chamfer

py	With chamfer, operator, height 4,Smm(.177). or large illuminated ring only
PZ	Flat.operator height 4,Smm(.177). or large illuminated ring only
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)FINGER PRESSURE
applied to switch

1 = pressure
0 = no pressure


OUTPUT

· Momentary NO (pulse)
No external power supply required



· Momentary NO (pulse)
No external power supply required


· Momentary NO prolongated pulse
No external power supply required


· Latching (ON-OFF)
Requires external power supply
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)Wiring diagrams

1 = closed output	O = opeb output
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)Legend:B = black, A= same colour as LED
*LED colour is indicated by the bottom of the product.
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