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Product Description

Features:
· A variety of styles to choose from:Flat/Chamfer/Concave
· Glued Package IP68 waterproof pure copper wire,good conductivity
. Waterproof,dustproof,flame retardant head waterproof and dustproof flame retardant plastic parts
· LED high light wicks,LED life can reach 30,000 hours bright color,soft bright,long life
· The LED indicators are available in a variety of colors



	Product Name
	IP68 Waterproof Piezo Switch

	Model
	ZMPS30A-H1OM
	ZMPS30A-H10M/D
	ZMPS30A-D10M/R

	Mounting Hole Size
	30mm

	Operation Types
	Momentary (Reset)

	Switch Combination
	1NO

	Actuator Shape
	Flat/Chamfer/Concave/High  Flat

	Terminal type
	Wired lead

	Illuminated or not
	Yes or NO

	Led Voltage
	3-24V

	Led Color
	Blue (Red,Green,  Yellow,White,Orange,Purple available)

	Illuminated Type
	Ring/Dot

	Enclosure Material
	Stainless Steel/ Aluminum

	Rated Current
	2A

	Contact Resistance
	50 mn max

	Operating Force
	6 to 15N

	Dielectric Intensity
	2000VAC

	Operating Temperature
	-40°C to +75°C

	Accessories
	Nut, Rubber Waterproof O-ring

	Customized symbol,colored housing or Connector
	Acceptable and with fast shipping

	Choose 2/3 colors from two-color/three-color light combination (above colors)


Note: Dot lights are only available in the first 5 colors
Product Parameter


<1>33.00 (1.299DIA)
 (
I
...........,
,
 
 
----=--,.....-,
 
oco
(')
.
-
:::
,t
<1>28.50
(1.122D!A)
) (
<D
30.00
 
x
 
1
.00
 
S
I
I
_
(1.181DIAx1.001S
)
...
)E;:::I	::t===t

<1>33.00 (1.299D!A)

<1>27.00 (1.063D!A)




i	----+----=-.		, 0:

;:-1

 (
<1>28.50 
(1.122D!A)
) (
000
LO
 
(I')
,..............
 
--'----,
  
o,-
...
-
U'),....
,q
·
-
-
.._;,
)cr>.f.'.-.;.,

, --=--.,........... -










0 -
0,-...
C\1--0

<1>35.00 (1.3780IA)











 (
3.50
(.138
)
<I>
30.00
x
 
1.00SI
 
-
>
,0.
(1.1810IAx
 
1
.
00IS)
AWG26
30CM
) (
►
)<1>33.00
(1.2990IA)4

i		._---+----=-........ , o-

ZMPS30A-H1OM
<1>33.00
 (
,
.
) (
►
)(1.2990IA)
 (
o
O
-
 
)t
.
-
.
,
,
II)
 
:g
----'-------
=:;..............
-
....
  
----.------
=,,
..........
00)
0
.
 
-
(')
·-
0
DIA)
.50
256)
)1





<1>27.00
 (
O<D
C\I
 
C\I
('
·
-
)
  
.
)[image: ][image: ]  (1.0630IA)	






- ....:,	,,

.---'------'='-....,.	,









IED
<!>3.0
(.118


...;.



<!>30.00 x 1.00SI -C	of.
{1181D1Ax1.00IS)@iil.;J I
[image: ]AWG26
 30CM	




ZMPS30A-D1OM/R


6
{.


ZMPS30A-H1OM/D
image6.jpeg




image7.jpeg




image8.png




image9.jpeg




image10.jpeg




image11.jpeg




image12.jpeg
*

D

D)

=




image13.jpeg
(viasos’)
0591 ®




image14.jpeg
TL;JW

(1.122D1A) o
R8
¥z

Il 4
Q.

13.50
(.531DIA)





image15.jpeg
(via602)
05910




image16.jpeg
®13.50
(.531DIA)





image17.jpeg




image18.jpeg




image1.jpeg




image2.jpeg




image3.jpeg




image4.png




image5.jpeg




